ADC Interface FPGA IP

Revision: 1.0

Date: 21 Aug 2020

QuickLogic Corporation

# Requirement:

1. Interface with Analog devices chip AD7476A (12-bit ADC)
2. Fast throughput rate: 1 MSPS

# System Block Diagram:



# Pinout (for the QuickFeather board):

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Signal Name** | **eFPGA port # (S3B device)** | **QFN package pin** | **QuickFeather J8 connector** | **PMOD Interface Type 2 (SPI)** | **Direction** | **Description** |
| CSn\_o | IO\_31 | 23 | J8.5 | Pin 1 | Output | Slave Select, Active Low |
| SCLK\_o | IO\_7 | 63 | J8.11 | Pin 4 | Output | SPI Clock |
| SDATA\_i | IO\_5 | 64 | J8.9 | Pin 3 | Input | MISO |
| SDATA\_o | IO\_12 | 56 | J8.7 | Pin 2 | Output | MOSI, unused |
| GND\_o | IO\_10 | 59 | J8.13 | Pin 5 | Output | GND, required on PMOD connector |
|  |  |  | J8.15 | Pin 6 |  | VCC |

# Address Map Specification

## Memory Map

The EOS 3B system maps the FPGA IP into the address range of 0x40020000 to 0x4003FFFF. This address range provides 128K bytes of address range for FPGA based IP. The following tables further define the registers within this range.

Table 1‑1: FPGA IP Register Space

|  |  |  |  |
| --- | --- | --- | --- |
| Register | Block | Space Allocated | Remarks |
| 0x40020000 – 0x400200FF | FPGA IP Registers | 256 bytes |  |
| 0x40020100 – 0x4002FFFF | Reserved | 0x0 |  |
| 0x40030000 – 0x40030FFF | DMA control/Status registers | 1024 Words | Dedicated DMA registers |
| 0x40031000 – 0x40031FFF | DMA CH0 Port register | 1024 Words | Dedicated 4KB space for DMA Channel 0 |
| 0x40032000 – 0x4003FFFF | Reserved | 0x0 |  |

## Register Address Table

The following sections will outline the expected allocation of registers and describe their operations.

### FPGA Registers Address Table

Table 1‑2 shows the expected allocation of FPGA Registers address space.

Table 1‑2: FPGA IP Register Table

| Register | Block | Reset Value | Remarks |
| --- | --- | --- | --- |
| 0x40020000 | IP Device ID | 0x0ADC0001 | Read only |
| 0x40020004 | IP Revision number | 0x00000100 | Read only  Version 1.0 |
| 0x40020008 | FIFO Flush | 0x00 |  |
| 0x4002000C | Sensor Enable Register | 0x0 | Read/Write |
| 0x40020010 – 0x400200FF | Not Used | 0x0 |  |
| 0x40020100 – 0x4002FFFF | Reserved | 0x0 |  |
| 0x40030000 | DMA Enable Register | 0x0 | Read/Write |
| 0x40030004 | DMA Status Register | 0x0 | Read only |
| 0x40030008 | DMA Interrupt Enable Register | 0x0 | Read/Write |
| 0x4003000C – 0x40030FFF | Not Used | 0x0 |  |
| 0x40031000 | DMA Read Port register | 0x0 | Read only |
| 0x40031004 – 0x40031FFF | Not Used | 0x0 |  |
| 0x40032000 – 0x4003FFFF | Reserved | 0x0 |  |

## Description of Registers

The following sections will detail the registers for each address space.

### Conventions

| Access Tag | Name | Meaning |
| --- | --- | --- |
| R | Read | field may be read by the user/sw |
| W | Write | field may be written by the user/sw |
| U | Update | field may be updated by hardware |
| S | Set | field may be set by the user |
| C | Clear | field may be cleared by the user |
| RO | Read Only | field can only be read by the user/sw |

### FPGA IP Registers

#### IP Device ID register

Register Address location: 0x40020000

Reset Value: 0x0ADC0001

Table 1‑3.1: ID Value Register

|  |  |  |  |
| --- | --- | --- | --- |
| Name | Bit(s) | Type | Description |
| IP Device ID | [31:0] | RO | 0x0ADC0001 : Read only |

#### 

#### IP revision number register

Register Address location: 0x40020004

Reset Value: 0x0100

Table 1‑3.2: Revision Number Register

|  |  |  |  |
| --- | --- | --- | --- |
| Name | Bit(s) | Type | Description |
| Revision Number | [15: 0] | RW | 0x0100 : Read only |
| Not Used | [31:16] | RO | Return “0” when read |

#### FIFO Reset Register

Register Address location: 0x40020008

Reset Value: 0x0

Table 1‑3.3: FIFO Reset Register

|  |  |  |  |
| --- | --- | --- | --- |
| Name | Bit(s) | Type | Description |
| FIFO Reset | [0] | RW | RX FIFO Flush  HW auto clear |
| Not Used | [31:1] | RO | Return “0” when read |

#### Sensor Enable Register

Register Address location: 0x4002000C

Reset Value: 0x0

Table 1‑3.4: Sensor Enable Register

| Name | Bit(s) | Type | Description |
| --- | --- | --- | --- |
| Sensor 1 Enable | [0] | R/W | 0 – Sensor Disabled  1 – Sensor Enabled  When enabled the IP starts reading from the ADC |
| Reserved | [31:4] | R | Return “0” when read |

#### DMA Enable Register

Register Address location: 0x40030000

Reset Value: 0x00

Table 1‑3.11: DMA Enable Register

| Name | Bit(s) | Type | Description |
| --- | --- | --- | --- |
| DMA CH0 Enable | [0] | R/W | DMA Enable For channel 0  0 – Disable  1 – Enable  HW clears this bit when the DMA transfer is done.  DMA for reading the Sensor data. |
| Reserved | [31:1] | R | Returns “0” |

#### DMA Status Register

Register Address location: 0x40030004

Reset Value: 0x00

Table 1‑3.12: DMA Status Register

| Name | Bit(s) | Type | Description |
| --- | --- | --- | --- |
| DMA Done Interrupt | [0] | R/W | DMA Read Done Interrupt  FW needs to clear the interrupt, write 0 to clear. |
| Reserved | [31:1] | R | Returns “0” |

#### DMA Interrupt Enable Register

Register Address location: 0x40030008

Reset Value: 0x00

Table 1‑3.13: DMA Interrupt Enable Register

| Name | Bit(s) | Type | Description |
| --- | --- | --- | --- |
| DMA Done Interrupt Enable | [0] | R/W | 0 – disable  1 – enable. |
| Reserved | [31:1] | R | Returns “0” |

#### DMA CH0 Data Port Register (Read Port)

Register Address location: 0x40031000

Reset Value: 0x00

Table 1‑3.14: DMA CH0 Data Port Register (Read Port)

| Name | Bit(s) | Type | Description |
| --- | --- | --- | --- |
| DMA CH0 Port | [31:0] | R | DMA CH0 Port (Read Port)  RX FIFO Read Port |

# Programming steps:

1. Reset FIFO
2. M4 sets up DMA CH0 (FPGA Channel12) for Reading the Sensor data
3. M4 Enables the DMA for CH0
4. M4 Programs the Sensor Enable Register (0x4002000C)
5. When Sensor Enabled, FPGA IP reads the data from the AD7476A device and writes into the RX FIFO.
6. FPGA IP generates DREQ to the SDMA controller to read the data
7. When Read DMA is complete DMA Done Interrupt is generated
8. M4 repeats step 2 to 3 to set up the next DMA and capture the sensor data
9. FPGA IP continues to read the Data from AD7476A device till the Sensor is Enabled

# Data Format (32 -bit DMA):

Sensor data:

|  |  |
| --- | --- |
| **Sensor Data1 [15:0]** | **Sensor Data0 [15:0]** |
| **Sensor Data3 [15:0]** | **Sensor Data2 [15:0]** |
| **Sensor Data5 [15:0]** | **Sensor Data4 [15:0]** |
| **Sensor Data7 [15:0]** | **Sensor Data6 [15:0]** |
| **.** | **.** |
| **.** | **.** |

# Revision History

|  |  |  |  |
| --- | --- | --- | --- |
| **Date** | **Revision** | **Author** | **Description** |
| 21 Aug 2020 | 1.0 | Randy O | Copied from a previous customer design. Modified for the QuickFeather board. Changed the device and revision ID’s, modified pinout table in section 3. |

# Copyright and Trademark Information

All trademarks and / or trade names are property of their respective owners.

The information in this specification has been carefully reviewed for technical accuracy. However, QuickLogic does not take the responsibility for the accuracy of the included information. Quicklogic will not be held liable for damages which result from relying on the accuracy of the information contained in this specification. This specification is subject to change without notification.

If you find any errors or require additional explanation, please inform Quicklogic. All trademarks and / or trade names are property of their respective owners.

Copyright © 2016 QuickLogic

All rights reserved.

QuickLogic Corporation

2220 Lundy Ave.

Sunnyvale CA. 95131, USA