AEC FPGA Project

Revision: 1.01

Date: 16 Feb 2021

QuickLogic Corporation

# Requirement:

# Pinout:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Sl. No.** | **Signal Name** | **PAD Number** | **Direction** | **Description** |
| FLL | | | | |
| 1 | I2S\_bitclk\_in |  | Input |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

# FPGA Interrupts:

|  |  |  |
| --- | --- | --- |
| **Sl. No.** | **FPGA Interrupts to M4** | **Interrupt Description** |
| 1 | FB\_INTERRUPT\_0 | Local clock slow down |
| 2 | FB\_INTERRUPT\_1 | Local clock speed up |
| 3 | FB\_INTERRUPT\_2 | I2S Interrupt |
| 4 | FB\_INTERRUPT\_3 | Reserved |

Note: The I2S Interrupt is a combination of the following interrupts, logically OR’ed together:

* I2S Disconnected Interrupt
* I2S DMA Done Interrupt
* I2S Decimation Done Interrupt
* I2S Decimation DMA Start Interrupt

To determine the source of an I2S Interrupt, firmware must inspect the I2S Slave RX register module’s Interrupt Status register. Refer to the I2S Slave RX Register document in QuickLogic’s s3-gateware repository, under the /ip\_modules/I2S\_slave\_rx/ directory. The individual interrupts that may trigger an I2S Interrupt as described above may be individually enabled via the register at offset 0x100C in the I2S Slave RX IP module (offset 0x100C from the FPGA’s address offset + the I2S Slave RX module’s offset). Likewise, the status of the individual interrupts may be seen in the register at offset 0x1008 in the I2S Slave RX IP module (offset 0x1008 from the FPGA’s address offset + the I2S Slave RX module’s offset). The source of each interrupt may also be cleared by writing to the interrupt status register as described in the I2S Slave RX Register Document. Further details are listed below:

* I2S Disconnected Interrupt
  + Enabled via Interrupt Enable Register (0x100C), bit 3
  + Status/Clear via Interrupt Status Register (0x1008), bit 3
* I2S DMA Done Interrupt
  + Enabled via Interrupt Enable Register (0x100C), bit 0
  + Status/Clear via Interrupt Status Register (0x1008), bit 0
* I2S Decimation Done Interrupt
  + Enabled via Interrupt Enable Register (0x100C), bit 2
  + Status/Clear via Interrupt Status Register (0x1008), bit 2
* I2S Decimation DMA Start Interrupt
  + Active when the Decimation RX FIFO level (viewable at offset 0x1010) is greater than or equal to the DMA Count Register (0x1028). Note that unlike the other interrupts listed above, this interrupt does not have an enable/status bit.

# FPGA Clocks

The FPGA clock C16 should be set to 6MHz (1024\*6000). The FPGA clock C21 should be set to 3MHz (1024\*3000). The 6MHz clock is used by the decimation filter, and the 3MHz clock is used as the local I2S bit clock.

# Address Map Specification

## Memory Map

The EOS 3B system maps the FPGA IP into the address range of 0x40020000 to 0x4003FFFF. This address range provides 128K bytes of address range for FPGA based IP. The following tables further define the registers within this range.

Table 1‑1: FPGA IP Register Space

|  |  |  |  |
| --- | --- | --- | --- |
| Register | Block | Space Allocated | Remarks |
| 0x40020000 – 0x400200FF | FPGA IP Registers | 256 bytes |  |
| 0x40020100 – 0x40020FFF | Reserved |  |  |
| 0x40021000 – 0x40021FFF | FLL\_I2S | 4096 bytes |  |
| 0x40022000 – 0x40024FFF | I2S Slave RX (includes decimator) | 8192 bytes |  |
| 0x40025000 – 0x4003FFFF | Reserved |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

## Register Address Table

The following sections will outline the expected allocation of registers and describe their operations.

### FPGA Registers Address Table

Table 1‑2 shows the expected allocation of FPGA Registers address space.

Table 1‑2: FPGA IP Register Table

| Register | Block | Reset Value | Remarks |
| --- | --- | --- | --- |
| 0x40020000 | IP Device ID | 0xABCD0200 | Read only |
| 0x40020004 | IP Revision number | 0x0100 | Read only  Version |
| 0x40020008 – 0x400200FF | Not Used | 0x0 | Reserved. |

### FLL\_I2S Register Map

The FLL\_I2S module has a base address that starts at offset 0x1000 from the FPGA’s base address (0x40020000 + 0x1000). The register map for the FLL\_I2S Controller is described in a separate document, and can be found along with the RTL source code for the FLL\_I2S module (currently in QuickLogic’s s3-gateware repository on github, under ip\_modules).

### I2S RAM and I2S Slave Register Map

The I2S Slave module has a base address that starts at offset 0x2000 from the FPGA’s base address (0x40020000 + 0x2000). The I2S RAM starts at offset 0x2000 from the FPGA’s base address, and the I2S Slave registers start at offset 0x3000 from the FPGA’s base address. The register map for the I2S Slave Controller is described in a separate document, and can be found along with the RTL source code for the I2S Slave module (currently in QuickLogic’s s3-gateware repository on github, under ip\_modules).

### FIR Coefficients Register Map

The 3to1 Decimation (FIR) Filter module has a base address that starts at offset 0x4000 from the FPGA’s base address (0x40020000 + 0x4000). The register map for the Decimation Filter is described in a separate document, and can be found along with the RTL source code for the I2S Slave module (currently in QuickLogic’s s3-gateware repository on github, under ip\_modules).

# Revision History

|  |  |  |  |
| --- | --- | --- | --- |
| **Date** | **Revision** | **Author** | **Description** |
| 21 Jan 2021 | 1.00 | Randy O. | Initial Release |
| 16 Feb 2021 | 1.01 | Randy O. | Added clock requirements |
|  |  |  |  |

# Copyright and Trademark Information

All trademarks and / or trade names are property of their respective owners.

The information in this specification has been carefully reviewed for technical accuracy. However, QuickLogic does not take the responsibility for the accuracy of the included information. Quicklogic will not be held liable for damages which result from relying on the accuracy of the information contained in this specification. This specification is subject to change without notification.

If you find any errors or require additional explanation, please inform Quicklogic. All trademarks and / or trade names are property of their respective owners.

Copyright © 2020 QuickLogic

All rights reserved.

QuickLogic Corporation

2220 Lunday Ave.

San Jose CA. 95131, USA