UART FPGA IP

Revision: 1.01

Date: 21 Sep 2020

QuickLogic Corporation

# Requirement:

# Pinout:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Sl. No.** | **Signal Name** | **PAD Number** | **Direction** | **Description** |
| **UART** | | | | |
| 4 | UART\_TX |  | Output |  |
| 5 | UART\_RX |  | Input |  |

# FPGA Interrupts:

|  |  |  |
| --- | --- | --- |
| **Sl. No.** | **FPGA Interrupts to M4** | **Interrupt Description** |
| 1 | FB\_INTERRUPT\_0 | Reserved |
| 2 | FB\_INTERRUPT\_1 | Reserved |
| 3 | FB\_INTERRUPT\_2 | UART 0 INTR |
| 4 | FB\_INTERRUPT\_3 | UART 1 INTR |

# Address Map Specification

## Memory Map

The EOS 3B system maps the FPGA IP into the address range of 0x40020000 to 0x4003FFFF. This address range provides 128K bytes of address range for FPGA based IP. The following tables further define the registers within this range.

Table 1‑1: FPGA IP Register Space

|  |  |  |  |
| --- | --- | --- | --- |
| Register | Block | Space Allocated | Remarks |
| 0x40020000 – 0x400200FF | FPGA IP Registers | 256 bytes |  |
| 0x40020100 – 0x40020FFF | Reserved | 0x0 |  |
| 0x40021000 – 0x400217FF | UART 0 | 512 Words |  |
| 0x40022000 – 0x400227FF | UART 1 | 512 Words |  |
| 0x40022800 – 0x4003FFFF | Reserved | 0x0 |  |

## Register Address Table

The following sections will outline the expected allocation of registers and describe their operations.

### FPGA Registers Address Table

Table 1‑2 shows the expected allocation of FPGA Registers address space.

Table 1‑2: FPGA IP Register Table

| Register | Block | Reset Value | Remarks |
| --- | --- | --- | --- |
| 0x40020000 | IP Device ID | 0xABCD0002 | Read only |
| 0x40020004 | IP Revision number | 0x0100 | Read only  Version |
| 0x40020008 – 0x400200FF | Not Used | 0x0 |  |

### UART 0 and UART 1 Address Map

UART 0 has a base address that starts at offset 0x1000 from the FPGA’s base address (0x40020000 + 0x1000). UART 1 has a base address that starts at offset 0x2000 from the FPGA’s base address (0x40020000 + 0x2000). The register map for each UART is described in a separate document, and can be found along with the RTL source code for the UART (currently in QuickLogic’s s3-gateware repository on github, under ip\_modules).

# Revision History

|  |  |  |  |
| --- | --- | --- | --- |
| **Date** | **Revision** | **Author** | **Description** |
| 17 Sep 2020 | 1.00 | Randy O | Initial Release |
| 21 Sep 2020 | 1.01 | Randy O | Removed the UART register map, since it’s now described in a separate document. Updated QuickLogic’s address. |
|  |  |  |  |
|  |  |  |  |

# Copyright and Trademark Information

All trademarks and / or trade names are property of their respective owners.

The information in this specification has been carefully reviewed for technical accuracy. However, QuickLogic does not take the responsibility for the accuracy of the included information. Quicklogic will not be held liable for damages which result from relying on the accuracy of the information contained in this specification. This specification is subject to change without notification.

If you find any errors or require additional explanation, please inform Quicklogic. All trademarks and / or trade names are property of their respective owners.

Copyright © 2020 QuickLogic

All rights reserved.

QuickLogic Corporation

2220 Lunday Ave.

San Jose CA. 95131, USA